start

Converter List

Converter list window will list all TCP/IP converters on the LAN where the computer located. Each converter use MAC address display.
Notice: Before setup, please connect all converters on LAN (Do not cross any gateway). If new controller is connected on LAN, please click this window tools "Search Converter" Button.
To setup converter, please select one or more converters in the list first, then change and save the property in the "property" window. For instruction, please refer to Select Method. User can setup multi-controllers at the same time when they are selected.
Why converter connected is not listed?
Possible reasons are:
1. Converter is not Anson model. To setup it, please refer to user manual.
2. Converter and computer are not in the same LAN. Converter and computer can cross HUB and simple router, but can not cross gateway.
3. After power on converter or update setup, converter will start to work within 5s.

Move mouse cursor on the list and right click then the command menu will pop up, which includes following orders:
1. Select all
Function: Select all items in the list.
2. Reversed Select
Function: Select all items that have not been selected in the list.
3. Detail Setup
Function: Setup more parameters in converter setup program.
This command may require user inputting converter user name and password. The default user name and password are "admin". Acquire more detailed setup information.
Tool Button Instruction
Search Converter
Search converter on LAN again.
Cancel operation
Cancel current operations. The button is unusable, when there is no operation.