start

Network Controller Setup

If controller connects with computer network by controller built-in TCP/IP network port, user must setup the controller IP address, Subnet Mask and gateway.
Notice: Before setup, please connect all controllers on LAN where computer located (Do not cross any gateway). If controller and computer are not in the same network, please connect the controller on LAN and setup it firstly. After setup completed, connect the controller to target network.
To find out detailed information of any item in the window, please click the item.