start

Monitor Map Window

The window can display but not edit the E-map opened. The monitoring point will flash when there is any event. If a reader in a map is set as "Remote Authentication" in window "Door", "Remote open" dialog box will pop up when user presents card or inputs password. If user press "Yes" within 10s, the door will be opened.
Monitoring point instruction:
stands for reader monitoring point.stands for door monitoring point. stands for alarm input monitoring point. stands for exit button monitoring point.
To edit E-map, please go to window "Monitor-edit mode"..
When display monitoring point, select the monitoring point and do not release it. Then move the mouse to " and release it in the targeted location.
Notice: One monitoring point can only link with one video channel. But one video channel can link with multi-monitoring points. So when one monitoring point links with another video channel, the original linkage relation will be deleted.

For toolbar button instruction, please refer to "map monitor toolbar".