start

Network Controller List

Network controller list window will list all network controllers on the LAN where computer located. Each network controller is represented by its MAC address.
Notice: Before setup, please connect all network controllers on LAN where computer located (Do not cross any gateway). If new network controller is connected on LAN, please click "Search Converter" Button.
To setup network controller, please select one or more controllers in the list firstly, then change and save the property in the "property" window. Instruction for selection, please refer to Select Method. User can setup multi-controllers at the same time, when they are selected.
Why connected network controller can not be listed?
Possible reasons are:
1 The controller is note supported by the software.
2 Controller and computer are not in the same LAN. Controller and computer can cross HUB and simple router, but can not cross gateway.
3 After power on controller or update setup, controller will start to work within 5s.

In the list right click the mouse command menu will pop up. This menu includes following orders:
1. Select all
Function: Select all items in the list.
2. Reversed Select
Function: Select all items that have not been selected in the list.
Toolbar Button Instruction
Search Network Controller
Search network controller in LAN again
Cancel Operation
Cancel current operations. The button is unusable, when there is no operation.