start

Converter Setup

If controller connects with computer network by TCP/IP communication converter, user must setup controller IP address, subnet mask and gateway. If user use Anson converter, user just setup it in this window directly.
Notice: Before setup, please connect all converters on LAN (Do not cross any gateway). If converter and computer are not in the same network, please connect the converter on LAN and setup it firstly. After setup completed, connect the converter to target network.
One converter 485 port can connect with multi-controllers.
To find out detailed information of any item in the window, please click the item.