start

Monitor-edit Mode

The window is used in real-time monitoring E-map, user can edit multi-maps and save it. The window is only used in expert mode.
Notice: If computer is equipped with appointed video compression card, once software go to the window or "monitor-monitor mode", the software will detect and initialize all video compression channels. The detect time depends on compression card and the number of doors. So please wait patiently.
If user have opened map by "Monitor-edit mode" or "monitor-control mode" last time, the window will display last map, or it will be blank.
The software will monitor present card event and alarm event. Before start monitor, please edit an E-map. For example: select reader, door-magnet input, and alarm input and exit button for this map. You can also import a background, and then move all the monitoring points to certain positions. If computer is equipped with appointed video compression card, user can link monitoring point with video channel in the window.
To find out detailed information of any item in the window, please click the item.