start

Global Anti-passback Group Setup

Global anti-passback function is used among readers of different controllers. Readers from different controller can be added to one group. This is different from the general anti-passback of "controller" setup, only readers from the same controller can be added to one general anti-passback group.

If it is your first time to use global anti-passback function, please setup anti-passback network interface and service port in Options. Before setup new global anti-passback group, you need setup controller in "controller" view so that software can get reader information.

If you want to learn more about an element, please click the element.