start

Edit Map Window

The window displays and edits monitoring points and background of the map.
Monitoring Point Instruction:
stands for reader, to add password and card to the monitoring point.stands for door, to add door-magnet input to the monitoring point. stands for alarm input, to add controller alarm input to the monitoring point.stands for exit button, to add exit button event to the monitoring point.
How to add and delete monitoring point?
To add or delete monitoring point, please go to "Add and delete toolbar" button. Added monitoring point will be displayed in the window.
How to import background picture?
To import background picture, please go to "Assign background picture" button in the window.
How to move monitoring point?
When display monitoring point, please select the monitoring point and do not release it. Then user can move the mouse and release it at target location.
How to connect with monitoring point and video channel?
When display monitoring point, select the monitoring point and left lick the mouse, then drag the point to "Video Channel"video list and release mouse. When monitoring point name appears in video list, it is OK. Notice: One monitoring point can only link with one video channel. But one video channel can link with multi-monitoring points. So when one monitoring point link with another video channel, the original linkage relation will be deleted.

In window right click will pop up a menu, The commend includ following command:
1. New Map
Function: To build a new map.
2. Open Map
Function: Open map and try to edit.
3. Save
Function: To save current change. Only save map change
4. Save as
Function: Save the editing map as another new map, and the original map is still exist.
5. Delete Current Map
Function: To delete current map from database.
For toolbar instruction, please refer to"Map Edit Toolbar".