start

Alarm List

The monitored alarm record will display in this list, each row stands for a record.
List meaning:
Serial Number: Temporary record number only stands for monitoring record sequence.
Alarm Type: Display event type. It is:
Door-open Timeout --- Controller detects door open time is over than "Time of Door-open Timeout" plus "Door Lock delay" (Door-magnet input is used in door open detect)
Alarm input --- Controller detects alarm input.
Time: Event time, the format is YYYY-MM-DD hh:mm:ss, YYYY is year, MM is Month, DD is day, hh is hour, mm is minute, ss is second.
Controller: Event controller
Alarm position: Door open timeout event will display event-door, alarm input event will display alarm input name.